<?xml version="1.0" encoding="utf-8"?>
<ACAML xmlns="urn:schemas-agilent-com:acaml15" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">
	<Checksum Algorithm="MD5">
		<Value>ZWZx7wZbi+gylocn+Et7/g==</Value>
	</Checksum>
	<Doc ContentVersioned="false">
		<DocID>1c1ea77a-de61-4075-bd80-4c897dbb6af7</DocID>
		<DocInfo>
			<Description>Method ACAML</Description>
			<CreatedByUser>CHY5012209DTW01\Student</CreatedByUser>
			<CreatedByApplication>
				<AgilentApp>
					<Name>ChemStation</Name>
					<Version>2.197.0.0</Version>
				</AgilentApp>
			</CreatedByApplication>
			<CreationDate>2025-04-10T21:34:08.2-06:00</CreationDate>
			<ClientName>CHY5012209DTW01</ClientName>
		</DocInfo>
		<Content>
			<MethodConfiguration xsi:type="MethodConfigurationType" id="f2088cf5-ff57-4da3-a8e1-cd859ab3346c" ver="0">
				<MethodDescription>
					<Name>Method Configuration</Name>
					<ID>Method_Configuration</ID>
					<Section>
						<Name>Acquisition Method</Name>
						<ID>Acquisition_Method</ID>
						<Section>
							<Name>Agilent 8890 (GC)</Name>
							<ID>GC</ID>
							<Section>
								<Name>GC Summary</Name>
								<ID>SUMMARY</ID>
								<Parameter>
									<Name>Run Time</Name>
									<ID>RUN_TIME</ID>
									<Unit>min</Unit>
									<Value>25</Value>
								</Parameter>
								<Parameter>
									<Name>Post Run Time</Name>
									<ID>POSTRUN_TIME</ID>
									<Unit>min</Unit>
									<Value>0</Value>
								</Parameter>
							</Section>
							<Section>
								<Name>Oven</Name>
								<ID>OVEN</ID>
								<Section>
									<Name>Temperature</Name>
									<ID>TEMPERATURE</ID>
									<Parameter>
										<Name>Setpoint</Name>
										<ID>STATE</ID>
										<Value>On</Value>
									</Parameter>
									<Parameter>
										<Name>(Initial)</Name>
										<ID>INITIAL</ID>
										<Unit>°C</Unit>
										<Value>40</Value>
									</Parameter>
									<Parameter>
										<Name>Hold Time</Name>
										<ID>HOLD</ID>
										<Unit>min</Unit>
										<Value>3.2</Value>
									</Parameter>
									<Parameter>
										<Name>Post Run</Name>
										<ID>POSTRUN</ID>
										<Unit>°C</Unit>
										<Value>50</Value>
									</Parameter>
									<Table>
										<Name>Program</Name>
										<ID>RAMP</ID>
										<Row>
											<Parameter>
												<Name>Rate</Name>
												<ID>RATE</ID>
												<Unit>°C/min</Unit>
												<Value>25</Value>
											</Parameter>
											<Parameter>
												<Name>Value</Name>
												<ID>NEXT</ID>
												<Unit>°C</Unit>
												<Value>250</Value>
											</Parameter>
											<Parameter>
												<Name>Hold Time</Name>
												<ID>HOLD</ID>
												<Unit>min</Unit>
												<Value>13.4</Value>
											</Parameter>
										</Row>
									</Table>
								</Section>
								<Parameter>
									<Name>Equilibration Time</Name>
									<ID>EQUIL_TIME</ID>
									<Unit>min</Unit>
									<Value>1</Value>
								</Parameter>
								<Parameter>
									<Name>Max Temperature</Name>
									<ID>MAX_TEMPERATURE</ID>
									<Unit>°C</Unit>
									<Value>350</Value>
								</Parameter>
								<Parameter>
									<Name>Maximum Temperature Override</Name>
									<ID>MaxTempOverride</ID>
									<Unit />
									<Value>Disabled</Value>
								</Parameter>
								<Parameter>
									<Name>Slow Fan</Name>
									<ID>CR_SlowFan</ID>
									<Unit />
									<Value>Disabled</Value>
								</Parameter>
							</Section>
							<Section>
								<Name>ALS</Name>
								<ID>ALS</ID>
								<Section>
									<Name>Front Injector</Name>
									<ID>FRONTINJ</ID>
									<Parameter>
										<Name>Syringe Size</Name>
										<ID>SYRINGE_SIZE</ID>
										<Unit>μL</Unit>
										<Value>10</Value>
									</Parameter>
									<Parameter>
										<Name>Injection Volume</Name>
										<ID>INJ_VOL</ID>
										<Unit>μL</Unit>
										<Value>1</Value>
									</Parameter>
									<Parameter>
										<Name>Solvent A Washes (PreInj)</Name>
										<ID>SOLV_A_WASH_PRE</ID>
										<Unit />
										<Value>3</Value>
									</Parameter>
									<Parameter>
										<Name>Solvent A Washes (PostInj)</Name>
										<ID>SOLV_A_WASH_POST</ID>
										<Unit />
										<Value>3</Value>
									</Parameter>
									<Parameter>
										<Name>Solvent A Volume</Name>
										<ID>SOLV_A_VOL</ID>
										<Unit>μL</Unit>
										<Value>8</Value>
									</Parameter>
									<Parameter>
										<Name>Solvent B Washes (PreInj)</Name>
										<ID>SOLV_B_WASH_PRE</ID>
										<Unit />
										<Value>3</Value>
									</Parameter>
									<Parameter>
										<Name>Solvent B Washes (PostInj)</Name>
										<ID>SOLV_B_WASH_POST</ID>
										<Unit />
										<Value>3</Value>
									</Parameter>
									<Parameter>
										<Name>Solvent B Volume</Name>
										<ID>SOLV_B_VOL</ID>
										<Unit>μL</Unit>
										<Value>8</Value>
									</Parameter>
									<Parameter>
										<Name>Sample Washes</Name>
										<ID>SAMP_WASH</ID>
										<Unit />
										<Value>2</Value>
									</Parameter>
									<Parameter>
										<Name>Sample Wash Volume</Name>
										<ID>SAMP_WASH_VOL</ID>
										<Unit>μL</Unit>
										<Value>2</Value>
									</Parameter>
									<Parameter>
										<Name>Sample Pumps</Name>
										<ID>SAMP_PUMPS</ID>
										<Unit />
										<Value>6</Value>
									</Parameter>
									<Parameter>
										<Name>Dwell Time (PreInj)</Name>
										<ID>DWELL_TIME_PRE</ID>
										<Unit>min</Unit>
										<Value>0</Value>
									</Parameter>
									<Parameter>
										<Name>Dwell Time (PostInj)</Name>
										<ID>DWELL_TIME_POST</ID>
										<Unit>min</Unit>
										<Value>0</Value>
									</Parameter>
									<Parameter>
										<Name>Solvent Wash Draw Speed</Name>
										<ID>SOLV_DRAW_SPEED</ID>
										<Unit>μL/min</Unit>
										<Value>300</Value>
									</Parameter>
									<Parameter>
										<Name>Solvent Wash Dispense Speed</Name>
										<ID>SOLV_DISP_SPEED</ID>
										<Unit>μL/min</Unit>
										<Value>3000</Value>
									</Parameter>
									<Parameter>
										<Name>Sample Wash Draw Speed</Name>
										<ID>SAMP_DRAW_SPEED</ID>
										<Unit>μL/min</Unit>
										<Value>300</Value>
									</Parameter>
									<Parameter>
										<Name>Sample Wash Dispense Speed</Name>
										<ID>SAMP_DISP_SPEED</ID>
										<Unit>μL/min</Unit>
										<Value>3000</Value>
									</Parameter>
									<Parameter>
										<Name>Injection Draw Speed</Name>
										<ID>INJ_DRAW_SPEED</ID>
										<Unit>μL/min</Unit>
										<Value>300</Value>
									</Parameter>
									<Parameter>
										<Name>Injection Dispense Speed</Name>
										<ID>INJ_DISP_SPEED</ID>
										<Unit>μL/min</Unit>
										<Value>6000</Value>
									</Parameter>
									<Parameter>
										<Name>Viscosity Delay</Name>
										<ID>VISCOSITY_DELAY</ID>
										<Unit>sec</Unit>
										<Value>2</Value>
									</Parameter>
									<Parameter>
										<Name>Sample Depth</Name>
										<ID>SAMP_DEPTH</ID>
										<Unit />
										<Value>Disabled</Value>
									</Parameter>
									<Parameter>
										<Name>Injection Type</Name>
										<ID>INJ_MODE</ID>
										<Unit />
										<Value>Standard</Value>
									</Parameter>
									<Parameter>
										<Name>L1 Airgap</Name>
										<ID>L1_AIRGAP</ID>
										<Unit>μL</Unit>
										<Value>0.2</Value>
									</Parameter>
									<Parameter>
										<Name>Solvent Wash Mode</Name>
										<ID>SOLV_WASHMODE</ID>
										<Unit />
										<Value>A, B</Value>
									</Parameter>
								</Section>
								<Section>
									<Name>Sample Overlap</Name>
									<ID>SAMP_OVERLAP</ID>
									<Parameter>
										<Name>Mode</Name>
										<ID>MODE</ID>
										<Unit />
										<Value>Sample overlap is not enabled</Value>
									</Parameter>
								</Section>
							</Section>
							<Section>
								<Name>Front SS Inlet H2</Name>
								<ID>INLET1</ID>
								<Parameter>
									<Name>Mode</Name>
									<ID>MODE</ID>
									<Unit />
									<Value>Split</Value>
								</Parameter>
								<Parameter>
									<Name>Heater</Name>
									<ID>HEATER</ID>
									<Unit>°C</Unit>
									<Value>On    250</Value>
								</Parameter>
								<Parameter>
									<Name>Pressure</Name>
									<ID>PRESSURE</ID>
									<Unit>psi</Unit>
									<Value>On    4.4452</Value>
								</Parameter>
								<Parameter>
									<Name>Total Flow</Name>
									<ID>TOTAL_FLOW</ID>
									<Unit>mL/min</Unit>
									<Value>On    38.7</Value>
								</Parameter>
								<Parameter>
									<Name>Septum Purge Flow</Name>
									<ID>SEPTUM_PURGE_FLOW</ID>
									<Unit>mL/min</Unit>
									<Value>On    3</Value>
								</Parameter>
								<Parameter>
									<Name>Pre-Run Flow Test</Name>
									<ID>INLET_LEAK_TEST</ID>
									<Unit />
									<Value>Off</Value>
								</Parameter>
								<Parameter>
									<Name>Gas Saver</Name>
									<ID>GAS_SAVER</ID>
									<Value>On    20 mL/min after 2 min</Value>
								</Parameter>
								<Parameter>
									<Name>Split Ratio</Name>
									<ID>SPLIT_RATIO</ID>
									<Unit>:1</Unit>
									<Value>50</Value>
								</Parameter>
								<Parameter>
									<Name>Split Flow</Name>
									<ID>SPLIT_FLOW</ID>
									<Unit>mL/min</Unit>
									<Value>35</Value>
								</Parameter>
								<Parameter>
									<Name>Liner</Name>
									<ID>LINER</ID>
									<Unit />
									<Value>A Liner has not been selected.</Value>
								</Parameter>
							</Section>
							<Section>
								<Name>Column</Name>
								<ID>COLUMN</ID>
								<Section>
									<Name>Column #1</Name>
									<ID>COLUMN1</ID>
									<Section>
										<Name>Flow</Name>
										<ID>FLOW</ID>
										<Parameter>
											<Name>Setpoint</Name>
											<ID>STATE</ID>
											<Value>On</Value>
										</Parameter>
										<Parameter>
											<Name>(Initial)</Name>
											<ID>INITIAL</ID>
											<Unit>mL/min</Unit>
											<Value>0.7</Value>
										</Parameter>
										<Parameter>
											<Name>Post Run</Name>
											<ID>POSTRUN</ID>
											<Unit>mL/min</Unit>
											<Value>1</Value>
										</Parameter>
									</Section>
									<Parameter>
										<Name>Column Information</Name>
										<ID>INFO</ID>
										<Value>Agilent 19091S-433UI: T330351H</Value>
									</Parameter>
									<Parameter>
										<Name>Description</Name>
										<ID>DESCRIPTION</ID>
										<Value>HP-5MS UI</Value>
									</Parameter>
									<Parameter>
										<Name>Temperature Range</Name>
										<ID>TEMPERATURERANGE</ID>
										<Value>-60 °C—325 °C (350 °C)</Value>
									</Parameter>
									<Parameter>
										<Name>Dimensions</Name>
										<ID>DIMENSIONS</ID>
										<Value>30 m x 250 μm x 0.25 μm (Uncalibrated)</Value>
									</Parameter>
									<Parameter>
										<Name>Heater</Name>
										<ID>HeatedBy</ID>
										<Value>Oven</Value>
									</Parameter>
									<Parameter>
										<Name>Column lock</Name>
										<ID>COLUMN_LOCKED</ID>
										<Unit />
										<Value>Locked</Value>
									</Parameter>
									<Parameter>
										<Name>In</Name>
										<ID>IN</ID>
										<Unit />
										<Value>Front SS Inlet H2</Value>
									</Parameter>
									<Parameter>
										<Name>Out</Name>
										<ID>OUT</ID>
										<Unit />
										<Value>Front Detector FID</Value>
									</Parameter>
									<Parameter>
										<Name>(Initial)</Name>
										<ID>INITIAL</ID>
										<Unit>°C</Unit>
										<Value>40</Value>
									</Parameter>
									<Parameter>
										<Name>Pressure</Name>
										<ID>PRESSURE</ID>
										<Unit>psi</Unit>
										<Value>4.4452</Value>
									</Parameter>
									<Parameter>
										<Name>Flow</Name>
										<ID>FLOW</ID>
										<Unit>mL/min</Unit>
										<Value>0.7</Value>
									</Parameter>
									<Parameter>
										<Name>Average Velocity</Name>
										<ID>VELOCITY</ID>
										<Unit>cm/sec</Unit>
										<Value>21.646</Value>
									</Parameter>
									<Parameter>
										<Name>Holdup Time</Name>
										<ID>HOLDUPTIME</ID>
										<Unit>min</Unit>
										<Value>2.3099</Value>
									</Parameter>
									<Parameter>
										<Name>Control Mode</Name>
										<ID>CONTROL_MODE</ID>
										<Unit />
										<Value>Constant Flow</Value>
									</Parameter>
								</Section>
								<Parameter>
									<Name>Column Outlet Pressure</Name>
									<ID>ColumnOutletPressure</ID>
									<Unit>psi</Unit>
									<Value>0</Value>
								</Parameter>
							</Section>
							<Section>
								<Name>Front Detector FID</Name>
								<ID>Detector 1</ID>
								<Parameter>
									<Name>Makeup</Name>
									<ID>MAKEUP</ID>
									<Unit />
									<Value>N2</Value>
								</Parameter>
								<Parameter>
									<Name>Heater</Name>
									<ID>Heater</ID>
									<Unit>°C</Unit>
									<Value>On    300</Value>
								</Parameter>
								<Parameter>
									<Name>H2 Flow (Combined)</Name>
									<ID>H2 Flow (Combined)</ID>
									<Unit>mL/min</Unit>
									<Value>On    30</Value>
								</Parameter>
								<Parameter>
									<Name>Air Flow</Name>
									<ID>Air Flow</ID>
									<Unit>mL/min</Unit>
									<Value>On    400</Value>
								</Parameter>
								<Parameter>
									<Name>Makeup Flow</Name>
									<ID>Makeup Flow</ID>
									<Unit>mL/min</Unit>
									<Value>On    20</Value>
								</Parameter>
								<Parameter>
									<Name>Carrier Gas Flow Correction</Name>
									<ID>CARRIER_GAS_CORRECTION</ID>
									<Unit />
									<Value>Column + Fuel = Constant</Value>
								</Parameter>
								<Parameter>
									<Name>Flame</Name>
									<ID>FLAME</ID>
									<Unit />
									<Value>On</Value>
								</Parameter>
								<Parameter>
									<Name>Blank Evaluation Setpoints</Name>
									<ID>BR_BLANK_RUN_SETPOINTS</ID>
									<Unit />
									<Value />
								</Parameter>
								<Parameter>
									<Name>Perform Blank Evaluation Test</Name>
									<ID>BR_PERFORM_BLANK_RUN_TEST</ID>
									<Unit />
									<Value>Off</Value>
								</Parameter>
							</Section>
							<Section>
								<Name>Detector Evaluation</Name>
								<ID>CA_HEADING</ID>
								<Parameter>
									<Name>Perform Detector Evaluation Test</Name>
									<ID>CA_PERFORM_ANALYSIS</ID>
									<Unit />
									<Value>Off</Value>
								</Parameter>
							</Section>
							<Section>
								<Name>Signals</Name>
								<ID>SIGNALS</ID>
								<Section>
									<Name>Signal #1:  Front Signal</Name>
									<ID>SIGNAL1</ID>
									<Parameter>
										<Name>Description</Name>
										<ID>DESCRIPTION</ID>
										<Unit />
										<Value>Front Signal</Value>
									</Parameter>
									<Parameter>
										<Name>Details</Name>
										<ID>DETAILS</ID>
										<Unit />
										<Value>Front Signal (FID)</Value>
									</Parameter>
									<Parameter>
										<Name>Save</Name>
										<ID>SAVE</ID>
										<Unit />
										<Value>On</Value>
									</Parameter>
									<Parameter>
										<Name>Data Rate</Name>
										<ID>DATA_RATE</ID>
										<Unit>Hz</Unit>
										<Value>5</Value>
									</Parameter>
									<Parameter>
										<Name>Dual Injection Assignment</Name>
										<ID>DUAL_ASSIGNMENT</ID>
										<Value>Front Sample</Value>
									</Parameter>
								</Section>
								<Section>
									<Name>Signal #2: </Name>
									<ID>SIGNAL2</ID>
									<Parameter>
										<Name>Description</Name>
										<ID>DESCRIPTION</ID>
										<Unit />
										<Value>None</Value>
									</Parameter>
								</Section>
								<Section>
									<Name>Signal #3: </Name>
									<ID>SIGNAL3</ID>
									<Parameter>
										<Name>Description</Name>
										<ID>DESCRIPTION</ID>
										<Unit />
										<Value>None</Value>
									</Parameter>
								</Section>
								<Section>
									<Name>Signal #4: </Name>
									<ID>SIGNAL4</ID>
									<Parameter>
										<Name>Description</Name>
										<ID>DESCRIPTION</ID>
										<Unit />
										<Value>None</Value>
									</Parameter>
								</Section>
								<Section>
									<Name>Signal #5: </Name>
									<ID>SIGNAL5</ID>
									<Parameter>
										<Name>Description</Name>
										<ID>DESCRIPTION</ID>
										<Unit />
										<Value>None</Value>
									</Parameter>
								</Section>
								<Section>
									<Name>Signal #6: </Name>
									<ID>SIGNAL6</ID>
									<Parameter>
										<Name>Description</Name>
										<ID>DESCRIPTION</ID>
										<Unit />
										<Value>None</Value>
									</Parameter>
								</Section>
								<Section>
									<Name>Signal #7: </Name>
									<ID>SIGNAL7</ID>
									<Parameter>
										<Name>Description</Name>
										<ID>DESCRIPTION</ID>
										<Unit />
										<Value>None</Value>
									</Parameter>
								</Section>
								<Section>
									<Name>Signal #8: </Name>
									<ID>SIGNAL8</ID>
									<Parameter>
										<Name>Description</Name>
										<ID>DESCRIPTION</ID>
										<Unit />
										<Value>None</Value>
									</Parameter>
								</Section>
							</Section>
						</Section>
						<Section>
							<Name>Agilent 8890</Name>
							<ID>Agilent8890</ID>
							<Section>
								<Name>GC</Name>
								<ID>GC</ID>
							</Section>
							<Section>
								<Name>GC Summary</Name>
								<ID>GCSummary</ID>
							</Section>
							<Section>
								<Name>Run Time                                     25 min</Name>
								<ID>RunTime25min</ID>
							</Section>
							<Section>
								<Name>Post Run Time                                0 min</Name>
								<ID>PostRunTime0min</ID>
							</Section>
							<Section>
								<Name>Oven</Name>
								<ID>Oven</ID>
							</Section>
							<Section>
								<Name>Temperature</Name>
								<ID>Temperature</ID>
							</Section>
							<Section>
								<Name>Setpoint                                     On</Name>
								<ID>SetpointOn</ID>
							</Section>
							<Section>
								<Name>(Initial)                                    40 °C</Name>
								<ID>(Initial)40°C</ID>
							</Section>
							<Section>
								<Name>Hold Time                                    3.2 min</Name>
								<ID>HoldTime3.2min</ID>
							</Section>
							<Section>
								<Name>Post Run                                     50 °C</Name>
								<ID>PostRun50°C</ID>
							</Section>
							<Section>
								<Name>Program</Name>
								<ID>Program</ID>
							</Section>
							<Section>
								<Name>#1 Rate                                      25 °C/min</Name>
								<ID>#1Rate25°C/min</ID>
							</Section>
							<Section>
								<Name>#1 Value                                     250 °C</Name>
								<ID>#1Value250°C</ID>
							</Section>
							<Section>
								<Name>#1 Hold Time                                 13.4 min</Name>
								<ID>#1HoldTime13.4min</ID>
							</Section>
							<Section>
								<Name>Equilibration Time                           1 min</Name>
								<ID>EquilibrationTime1min</ID>
							</Section>
							<Section>
								<Name>Max Temperature                              350 °C</Name>
								<ID>MaxTemperature350°C</ID>
							</Section>
							<Section>
								<Name>Maximum Temperature Override                 Disabled</Name>
								<ID>MaximumTemperatureOverrideDisabled</ID>
							</Section>
							<Section>
								<Name>Slow Fan                                     Disabled</Name>
								<ID>SlowFanDisabled</ID>
							</Section>
							<Section>
								<Name>ALS</Name>
								<ID>ALS</ID>
							</Section>
							<Section>
								<Name>Front Injector</Name>
								<ID>FrontInjector</ID>
							</Section>
							<Section>
								<Name>Syringe Size                                 10 μL</Name>
								<ID>SyringeSize10μL</ID>
							</Section>
							<Section>
								<Name>Injection Volume                             1 μL</Name>
								<ID>InjectionVolume1μL</ID>
							</Section>
							<Section>
								<Name>Solvent A Washes (PreInj)                    3</Name>
								<ID>SolventAWashes(PreInj)3</ID>
							</Section>
							<Section>
								<Name>Solvent A Washes (PostInj)                   3</Name>
								<ID>SolventAWashes(PostInj)3</ID>
							</Section>
							<Section>
								<Name>Solvent A Volume                             8 μL</Name>
								<ID>SolventAVolume8μL</ID>
							</Section>
							<Section>
								<Name>Solvent B Washes (PreInj)                    3</Name>
								<ID>SolventBWashes(PreInj)3</ID>
							</Section>
							<Section>
								<Name>Solvent B Washes (PostInj)                   3</Name>
								<ID>SolventBWashes(PostInj)3</ID>
							</Section>
							<Section>
								<Name>Solvent B Volume                             8 μL</Name>
								<ID>SolventBVolume8μL</ID>
							</Section>
							<Section>
								<Name>Sample Washes                                2</Name>
								<ID>SampleWashes2</ID>
							</Section>
							<Section>
								<Name>Sample Wash Volume                           2 μL</Name>
								<ID>SampleWashVolume2μL</ID>
							</Section>
							<Section>
								<Name>Sample Pumps                                 6</Name>
								<ID>SamplePumps6</ID>
							</Section>
							<Section>
								<Name>Dwell Time (PreInj)                          0 min</Name>
								<ID>DwellTime(PreInj)0min</ID>
							</Section>
							<Section>
								<Name>Dwell Time (PostInj)                         0 min</Name>
								<ID>DwellTime(PostInj)0min</ID>
							</Section>
							<Section>
								<Name>Solvent Wash Draw Speed                      300 μL/min</Name>
								<ID>SolventWashDrawSpeed300μL/min</ID>
							</Section>
							<Section>
								<Name>Solvent Wash Dispense Speed                  3000 μL/min</Name>
								<ID>SolventWashDispenseSpeed3000μL/min</ID>
							</Section>
							<Section>
								<Name>Sample Wash Draw Speed                       300 μL/min</Name>
								<ID>SampleWashDrawSpeed300μL/min</ID>
							</Section>
							<Section>
								<Name>Sample Wash Dispense Speed                   3000 μL/min</Name>
								<ID>SampleWashDispenseSpeed3000μL/min</ID>
							</Section>
							<Section>
								<Name>Injection Draw Speed                         300 μL/min</Name>
								<ID>InjectionDrawSpeed300μL/min</ID>
							</Section>
							<Section>
								<Name>Injection Dispense Speed                     6000 μL/min</Name>
								<ID>InjectionDispenseSpeed6000μL/min</ID>
							</Section>
							<Section>
								<Name>Viscosity Delay                              2 sec</Name>
								<ID>ViscosityDelay2sec</ID>
							</Section>
							<Section>
								<Name>Sample Depth                                 Disabled</Name>
								<ID>SampleDepthDisabled</ID>
							</Section>
							<Section>
								<Name>Injection Type                               Standard</Name>
								<ID>InjectionTypeStandard</ID>
							</Section>
							<Section>
								<Name>L1 Airgap                                    0.2 μL</Name>
								<ID>L1Airgap0.2μL</ID>
							</Section>
							<Section>
								<Name>Solvent Wash Mode                            A, B</Name>
								<ID>SolventWashModeA,B</ID>
							</Section>
							<Section>
								<Name>Sample Overlap</Name>
								<ID>SampleOverlap</ID>
							</Section>
							<Section>
								<Name>Mode                                         Sample overlap is not enabled</Name>
								<ID>ModeSampleoverlapisnotenabled</ID>
							</Section>
							<Section>
								<Name>Front SS Inlet H2</Name>
								<ID>FrontSSInletH2</ID>
							</Section>
							<Section>
								<Name>Mode                                         Split</Name>
								<ID>ModeSplit</ID>
							</Section>
							<Section>
								<Name>Heater                                       On    250 °C</Name>
								<ID>HeaterOn250°C</ID>
							</Section>
							<Section>
								<Name>Pressure                                     On    4.4452 psi</Name>
								<ID>PressureOn4.4452psi</ID>
							</Section>
							<Section>
								<Name>Total Flow                                   On    38.7 mL/min</Name>
								<ID>TotalFlowOn38.7mL/min</ID>
							</Section>
							<Section>
								<Name>Septum Purge Flow                            On    3 mL/min</Name>
								<ID>SeptumPurgeFlowOn3mL/min</ID>
							</Section>
							<Section>
								<Name>Pre-Run Flow Test                            Off</Name>
								<ID>Pre-RunFlowTestOff</ID>
							</Section>
							<Section>
								<Name>Gas Saver                                    On    20 mL/min after 2 min</Name>
								<ID>GasSaverOn20mL/minafter2min</ID>
								<Parameter>
									<Name>Split Ratio                                  50</Name>
									<ID>SplitRatio50</ID>
									<Unit />
									<Value>1</Value>
								</Parameter>
								<Parameter>
									<Name />
									<ID>SplitRatio50:1</ID>
									<Unit />
									<Value>Split Ratio                                  50 :1</Value>
								</Parameter>
							</Section>
							<Section>
								<Name>Split Flow                                   35 mL/min</Name>
								<ID>SplitFlow35mL/min</ID>
							</Section>
							<Section>
								<Name>Liner                                        A Liner has not been selected.</Name>
								<ID>LinerALinerhasnotbeenselected.</ID>
							</Section>
							<Section>
								<Name>Column</Name>
								<ID>Column</ID>
							</Section>
							<Section>
								<Name>Column #1</Name>
								<ID>Column#1</ID>
							</Section>
							<Section>
								<Name>Flow</Name>
								<ID>Flow</ID>
							</Section>
							<Section>
								<Name>Setpoint                                     On</Name>
								<ID>SetpointOn</ID>
							</Section>
							<Section>
								<Name>(Initial)                                    0.7 mL/min</Name>
								<ID>(Initial)0.7mL/min</ID>
							</Section>
							<Section>
								<Name>Post Run                                     1 mL/min</Name>
								<ID>PostRun1mL/min</ID>
								<Parameter>
									<Name>Column Information                           Agilent 19091S-433UI</Name>
									<ID>ColumnInformationAgilent19091S-433UI</ID>
									<Unit />
									<Value>T330351H</Value>
								</Parameter>
								<Parameter>
									<Name />
									<ID>ColumnInformationAgilent19091S-433UI:T330351H</ID>
									<Unit />
									<Value>Column Information                           Agilent 19091S-433UI: T330351H</Value>
								</Parameter>
							</Section>
							<Section>
								<Name>Description                                  HP-5MS UI</Name>
								<ID>DescriptionHP-5MSUI</ID>
							</Section>
							<Section>
								<Name>Temperature Range                            -60 °C—325 °C (350 °C)</Name>
								<ID>TemperatureRange-60°C—325°C(350°C)</ID>
							</Section>
							<Section>
								<Name>Dimensions                                   30 m x 250 μm x 0.25 μm (Uncalibrated)</Name>
								<ID>Dimensions30mx250μmx0.25μm(Uncalibrated)</ID>
							</Section>
							<Section>
								<Name>Heater                                       Oven</Name>
								<ID>HeaterOven</ID>
							</Section>
							<Section>
								<Name>Column lock                                  Locked</Name>
								<ID>ColumnlockLocked</ID>
							</Section>
							<Section>
								<Name>In                                           Front SS Inlet H2</Name>
								<ID>InFrontSSInletH2</ID>
							</Section>
							<Section>
								<Name>Out                                          Front Detector FID</Name>
								<ID>OutFrontDetectorFID</ID>
							</Section>
							<Section>
								<Name>(Initial)                                    40 °C</Name>
								<ID>(Initial)40°C</ID>
							</Section>
							<Section>
								<Name>Pressure                                     4.4452 psi</Name>
								<ID>Pressure4.4452psi</ID>
							</Section>
							<Section>
								<Name>Flow                                         0.7 mL/min</Name>
								<ID>Flow0.7mL/min</ID>
							</Section>
							<Section>
								<Name>Average Velocity                             21.646 cm/sec</Name>
								<ID>AverageVelocity21.646cm/sec</ID>
							</Section>
							<Section>
								<Name>Holdup Time                                  2.3099 min</Name>
								<ID>HoldupTime2.3099min</ID>
							</Section>
							<Section>
								<Name>Control Mode                                 Constant Flow</Name>
								<ID>ControlModeConstantFlow</ID>
							</Section>
							<Section>
								<Name>Column Outlet Pressure                       0 psi</Name>
								<ID>ColumnOutletPressure0psi</ID>
							</Section>
							<Section>
								<Name>Front Detector FID</Name>
								<ID>FrontDetectorFID</ID>
							</Section>
							<Section>
								<Name>Makeup                                       N2</Name>
								<ID>MakeupN2</ID>
							</Section>
							<Section>
								<Name>Heater                                       On    300 °C</Name>
								<ID>HeaterOn300°C</ID>
							</Section>
							<Section>
								<Name>H2 Flow (Combined)                           On    30 mL/min</Name>
								<ID>H2Flow(Combined)On30mL/min</ID>
							</Section>
							<Section>
								<Name>Air Flow                                     On    400 mL/min</Name>
								<ID>AirFlowOn400mL/min</ID>
							</Section>
							<Section>
								<Name>Makeup Flow                                  On    20 mL/min</Name>
								<ID>MakeupFlowOn20mL/min</ID>
							</Section>
							<Section>
								<Name>Carrier Gas Flow Correction                  Column + Fuel = Constant</Name>
								<ID>CarrierGasFlowCorrectionColumn+Fuel=Constant</ID>
							</Section>
							<Section>
								<Name>Flame                                        On</Name>
								<ID>FlameOn</ID>
							</Section>
							<Section>
								<Name>Blank Evaluation Setpoints</Name>
								<ID>BlankEvaluationSetpoints</ID>
							</Section>
							<Section>
								<Name>Perform Blank Evaluation Test                Off</Name>
								<ID>PerformBlankEvaluationTestOff</ID>
							</Section>
							<Section>
								<Name>Detector Evaluation</Name>
								<ID>DetectorEvaluation</ID>
							</Section>
							<Section>
								<Name>Perform Detector Evaluation Test             Off</Name>
								<ID>PerformDetectorEvaluationTestOff</ID>
							</Section>
							<Section>
								<Name>Signals</Name>
								<ID>Signals</ID>
								<Parameter>
									<Name>Signal #1</Name>
									<ID>Signal#1</ID>
									<Unit />
									<Value>Front Signal</Value>
								</Parameter>
								<Parameter>
									<Name />
									<ID>Signal#1:FrontSignal</ID>
									<Unit />
									<Value>Signal #1:  Front Signal</Value>
								</Parameter>
							</Section>
							<Section>
								<Name>Description                                  Front Signal</Name>
								<ID>DescriptionFrontSignal</ID>
							</Section>
							<Section>
								<Name>Details                                      Front Signal (FID)</Name>
								<ID>DetailsFrontSignal(FID)</ID>
							</Section>
							<Section>
								<Name>Save                                         On</Name>
								<ID>SaveOn</ID>
							</Section>
							<Section>
								<Name>Data Rate                                    5 Hz</Name>
								<ID>DataRate5Hz</ID>
							</Section>
							<Section>
								<Name>Dual Injection Assignment                    Front Sample</Name>
								<ID>DualInjectionAssignmentFrontSample</ID>
								<Parameter>
									<Name>Signal #2</Name>
									<ID>Signal#2</ID>
									<Unit />
									<Value />
								</Parameter>
								<Parameter>
									<Name />
									<ID>Signal#2:</ID>
									<Unit />
									<Value>Signal #2:</Value>
								</Parameter>
							</Section>
							<Section>
								<Name>Description                                  None</Name>
								<ID>DescriptionNone</ID>
								<Parameter>
									<Name>Signal #3</Name>
									<ID>Signal#3</ID>
									<Unit />
									<Value />
								</Parameter>
								<Parameter>
									<Name />
									<ID>Signal#3:</ID>
									<Unit />
									<Value>Signal #3:</Value>
								</Parameter>
							</Section>
							<Section>
								<Name>Description                                  None</Name>
								<ID>DescriptionNone</ID>
								<Parameter>
									<Name>Signal #4</Name>
									<ID>Signal#4</ID>
									<Unit />
									<Value />
								</Parameter>
								<Parameter>
									<Name />
									<ID>Signal#4:</ID>
									<Unit />
									<Value>Signal #4:</Value>
								</Parameter>
							</Section>
							<Section>
								<Name>Description                                  None</Name>
								<ID>DescriptionNone</ID>
								<Parameter>
									<Name>Signal #5</Name>
									<ID>Signal#5</ID>
									<Unit />
									<Value />
								</Parameter>
								<Parameter>
									<Name />
									<ID>Signal#5:</ID>
									<Unit />
									<Value>Signal #5:</Value>
								</Parameter>
							</Section>
							<Section>
								<Name>Description                                  None</Name>
								<ID>DescriptionNone</ID>
								<Parameter>
									<Name>Signal #6</Name>
									<ID>Signal#6</ID>
									<Unit />
									<Value />
								</Parameter>
								<Parameter>
									<Name />
									<ID>Signal#6:</ID>
									<Unit />
									<Value>Signal #6:</Value>
								</Parameter>
							</Section>
							<Section>
								<Name>Description                                  None</Name>
								<ID>DescriptionNone</ID>
								<Parameter>
									<Name>Signal #7</Name>
									<ID>Signal#7</ID>
									<Unit />
									<Value />
								</Parameter>
								<Parameter>
									<Name />
									<ID>Signal#7:</ID>
									<Unit />
									<Value>Signal #7:</Value>
								</Parameter>
							</Section>
							<Section>
								<Name>Description                                  None</Name>
								<ID>DescriptionNone</ID>
								<Parameter>
									<Name>Signal #8</Name>
									<ID>Signal#8</ID>
									<Unit />
									<Value />
								</Parameter>
								<Parameter>
									<Name />
									<ID>Signal#8:</ID>
									<Unit />
									<Value>Signal #8:</Value>
								</Parameter>
							</Section>
							<Parameter>
								<Name>Module Type</Name>
								<ID>ModuleType</ID>
								<Unit />
								<Value>GC</Value>
							</Parameter>
							<Parameter>
								<Name>Module Name</Name>
								<ID>ModuleName</ID>
								<Unit />
								<Value>Agilent 8890</Value>
							</Parameter>
						</Section>
						<Section>
							<Name>Column(s)</Name>
							<ID>Column(s)</ID>
							<Parameter>
								<Name>Column Description</Name>
								<ID>ColumnDescription</ID>
								<Unit />
								<Value>HP-5MS UI</Value>
							</Parameter>
							<Parameter>
								<Name>Inventory#</Name>
								<ID>Inventory#</ID>
								<Unit />
								<Value>T330351H</Value>
							</Parameter>
							<Parameter>
								<Name>Model#</Name>
								<ID>Model#</ID>
								<Unit />
								<Value>19091S-433UI</Value>
							</Parameter>
							<Parameter>
								<Name>Manufacturer</Name>
								<ID>Manufacturer</ID>
								<Unit />
								<Value>Agilent</Value>
							</Parameter>
							<Parameter>
								<Name>Diameter</Name>
								<ID>Diameter</ID>
								<Unit>µm</Unit>
								<Value>250.0</Value>
							</Parameter>
							<Parameter>
								<Name>Length</Name>
								<ID>Length</ID>
								<Unit>m</Unit>
								<Value>30.0</Value>
							</Parameter>
							<Parameter>
								<Name>Film thickness</Name>
								<ID>Filmthickness</ID>
								<Unit>µm</Unit>
								<Value>0.25</Value>
							</Parameter>
							<Parameter>
								<Name>Void time</Name>
								<ID>Voidtime</ID>
								<Unit>min</Unit>
								<Value>2.310</Value>
							</Parameter>
							<Parameter>
								<Name>Maximum Temperature</Name>
								<ID>MaximumTemperature</ID>
								<Unit>°C</Unit>
								<Value>325.0</Value>
							</Parameter>
							<Parameter>
								<Name>Comment</Name>
								<ID>Comment</ID>
								<Unit />
								<Value />
							</Parameter>
						</Section>
					</Section>
				</MethodDescription>
			</MethodConfiguration>
		</Content>
	</Doc>
</ACAML>
